# Microsemi Physical design constraints file

# Version: v11.4 11.4.0.112

# Design Name:  

# Input Netlist Format: EDIF 

# Family: SmartFusion2 , Die: M2S025T , Package: 484 FBGA , Speed grade: -1 

# Date generated: Fri Jul 18 14:09:42 2014 


#
# IO banks setting
#

set_iobank Bank2 -vcci 2.50 -fixed no
set_iobank Bank5 -vcci 2.50 -fixed no
set_iobank Bank6 -vcci 2.50 -fixed no
set_iobank Bank7 -vcci 2.50 -fixed no

#
# Local clock constraints
#


#
# Region constraints
#


#
# I/O constraints
#

set_io CLK0 -DIRECTION INPUT -pinname K1 -fixed yes
set_io DEVRST_N -DIRECTION INPUT -pinname R15
set_io GPIO_0_M2F -DIRECTION OUTPUT -pinname E1 -fixed yes
set_io GPIO_10_F2M -DIRECTION INPUT -pinname K21 -fixed yes
set_io GPIO_11_F2M -DIRECTION INPUT -pinname K20 -fixed yes
set_io GPIO_1_M2F -DIRECTION OUTPUT -pinname F4 -fixed yes
set_io GPIO_2_M2F -DIRECTION OUTPUT -pinname F3 -fixed yes
set_io GPIO_3_M2F -DIRECTION OUTPUT -pinname G7 -fixed yes
set_io GPIO_4_M2F -DIRECTION OUTPUT -pinname H7 -fixed yes
set_io GPIO_5_M2F -DIRECTION OUTPUT -pinname J6 -fixed yes
set_io GPIO_6_M2F -DIRECTION OUTPUT -pinname H6 -fixed yes
set_io GPIO_7_M2F -DIRECTION OUTPUT -pinname H5 -fixed yes
set_io GPIO_8_F2M -DIRECTION INPUT -pinname L19 -fixed yes
set_io GPIO_9_F2M -DIRECTION INPUT -pinname L18 -fixed yes
set_io REFCLK0_N -DIRECTION INPUT -pinname T1 -fixed yes
set_io REFCLK0_P -DIRECTION INPUT -pinname U1 -fixed yes
set_io RXD0_N -DIRECTION INPUT -pinname Y1
set_io RXD0_P -DIRECTION INPUT -pinname W1
set_io RXD1_N -DIRECTION INPUT -pinname Y3
set_io RXD1_P -DIRECTION INPUT -pinname W3
set_io RXD2_N -DIRECTION INPUT -pinname Y5
set_io RXD2_P -DIRECTION INPUT -pinname W5
set_io RXD3_N -DIRECTION INPUT -pinname Y7
set_io RXD3_P -DIRECTION INPUT -pinname W7
set_io SDIF0_PERST_N -DIRECTION INPUT -pinname P18 -fixed yes
set_io SWITCH -DIRECTION INPUT -pinname J18 -fixed yes
set_io TXD0_N -DIRECTION OUTPUT -pinname AA2
set_io TXD0_P -DIRECTION OUTPUT -pinname AB2
set_io TXD1_N -DIRECTION OUTPUT -pinname AA4
set_io TXD1_P -DIRECTION OUTPUT -pinname AB4
set_io TXD2_N -DIRECTION OUTPUT -pinname AA6
set_io TXD2_P -DIRECTION OUTPUT -pinname AB6
set_io TXD3_N -DIRECTION OUTPUT -pinname AA8
set_io TXD3_P -DIRECTION OUTPUT -pinname AB8

#
# Core cell constraints
#

