*****************************************************************
Pin Report - Date: Fri Jul 18 14:11:04 2014 Pinchecksum: NOT-AVAILABLE
Product: Designer
Release: v11.4
Version: 11.4.0.112
Design Name: PCIe_Demo_top
Family: SmartFusion2
Die: M2S025T
Package: 484 FBGA
*****************************************************************

Port          |Pin |Fixed |Function                       |Bank     |I/O Std   |Direction                      |I/O state in Flash*Freeze mode |Resistor Pull                      |I/O available in Flash*Freeze mode |Schmitt Trigger |Odt_Static    |Odt Imp (Ohm)  |Low Power Exit |Input Delay |Slew         |Pre-Emphasis      |Output Drive (mA) |Output Load (pF) |
--------------|----|------|-------------------------------|---------|----------|-------------------------------|-------------------------------|-----------------------------------|-----------------------------------|----------------|--------------|---------------|---------------|------------|-------------|------------------|------------------|-----------------|
CLK0           K1   Yes    MSIOD103PB6/CCC_SW0_CLKI0       Bank6     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
DEVRST_N       R15  Fixed  DEVRST_N                        ---       
GPIO_0_M2F     E1   Yes    MSIO89PB7                       Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
GPIO_1_M2F     F4   Yes    MSIO90NB7                       Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
GPIO_2_M2F     F3   Yes    MSIO90PB7                       Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
GPIO_3_M2F     G7   Yes    MSIO91NB7                       Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
GPIO_4_M2F     H7   Yes    MSIO91PB7                       Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
GPIO_5_M2F     J6   Yes    MSIO92NB7                       Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
GPIO_6_M2F     H6   Yes    MSIO92PB7                       Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
GPIO_7_M2F     H5   Yes    MSIO93NB7                       Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
GPIO_8_F2M     L19  Yes    MSIO18PB2/SPI_1_SS4/GPIO_17_A   Bank2     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
GPIO_9_F2M     L18  Yes    MSIO18NB2/SPI_1_SS5/GPIO_18_A   Bank2     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
GPIO_10_F2M    K21  Yes    MSIO19PB2/SPI_1_SS6/GPIO_23_A   Bank2     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
GPIO_11_F2M    K20  Yes    MSIO19NB2/SPI_1_SS7/GPIO_24_A   Bank2     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
REFCLK0_N      T1   Yes    MSIOD118NB5/SERDES_0_REFCLK0_N  Bank5     LVDS       Input                           TRISTATE                        None                                No                                  Off              Off            ---             ---             Off          ---           ---                ---                ---               
REFCLK0_P      U1   Yes    MSIOD118PB5/SERDES_0_REFCLK0_P  Bank5     LVDS       Input                           TRISTATE                        None                                No                                  Off              Off            ---             ---             Off          ---           ---                ---                ---               
RXD0_N         Y1   Fixed  SERDES_0_RXD0_N                 ---       
RXD0_P         W1   Fixed  SERDES_0_RXD0_P                 ---       
RXD1_N         Y3   Fixed  SERDES_0_RXD1_N                 ---       
RXD1_P         W3   Fixed  SERDES_0_RXD1_P                 ---       
RXD2_N         Y5   Fixed  SERDES_0_RXD2_N                 ---       
RXD2_P         W5   Fixed  SERDES_0_RXD2_P                 ---       
RXD3_N         Y7   Fixed  SERDES_0_RXD3_N                 ---       
RXD3_P         W7   Fixed  SERDES_0_RXD3_P                 ---       
SDIF0_PERST_N  P18  Yes    MSIO6NB2                        Bank2     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
SWITCH         J18  Yes    MSIO23NB2/SPI_1_SS3/GPIO_16_A   Bank2     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
TXD0_N         AA2  Fixed  SERDES_0_TXD0_N                 ---       
TXD0_P         AB2  Fixed  SERDES_0_TXD0_P                 ---       
TXD1_N         AA4  Fixed  SERDES_0_TXD1_N                 ---       
TXD1_P         AB4  Fixed  SERDES_0_TXD1_P                 ---       
TXD2_N         AA6  Fixed  SERDES_0_TXD2_N                 ---       
TXD2_P         AB6  Fixed  SERDES_0_TXD2_P                 ---       
TXD3_N         AA8  Fixed  SERDES_0_TXD3_N                 ---       
TXD3_P         AB8  Fixed  SERDES_0_TXD3_P                 ---       
