# Microsemi I/O Physical Design Constraints file
# Auto Generated User I/O Constraints file

# Version: v11.2 SP1 11.2.1.13
# Family: SmartFusion2 , Die: M2S050T , Package: 484 FBGA
# Date generated: Wed Feb 05 18:12:49 2014 


# 
# User Locked I/O Bank Settings
# 


# 
# Unlocked I/O Bank Settings
# The I/O Bank Settings can be locked by directly editing this file
# or by making changes in the I/O Attribute Editor
# 


# 
# User Locked I/O settings
# 

set_io CLK0           \
    -pinname K1       \
    -fixed yes        \
    -DIRECTION INPUT


set_io GPIO_0_M2F      \
    -pinname E1        \
    -fixed yes         \
    -DIRECTION OUTPUT


set_io GPIO_10_F2M    \
    -pinname K21      \
    -fixed yes        \
    -DIRECTION INPUT


set_io GPIO_11_F2M    \
    -pinname K20      \
    -fixed yes        \
    -DIRECTION INPUT


set_io GPIO_1_M2F      \
    -pinname F4        \
    -fixed yes         \
    -DIRECTION OUTPUT


set_io GPIO_2_M2F      \
    -pinname F3        \
    -fixed yes         \
    -DIRECTION OUTPUT


set_io GPIO_3_M2F      \
    -pinname G7        \
    -fixed yes         \
    -DIRECTION OUTPUT


set_io GPIO_4_M2F      \
    -pinname H7        \
    -fixed yes         \
    -DIRECTION OUTPUT


set_io GPIO_5_M2F      \
    -pinname J6        \
    -fixed yes         \
    -DIRECTION OUTPUT


set_io GPIO_6_M2F      \
    -pinname H6        \
    -fixed yes         \
    -DIRECTION OUTPUT


set_io GPIO_7_M2F      \
    -pinname H5        \
    -fixed yes         \
    -DIRECTION OUTPUT


set_io GPIO_8_F2M     \
    -pinname L19      \
    -fixed yes        \
    -DIRECTION INPUT


set_io GPIO_9_F2M     \
    -pinname L18      \
    -fixed yes        \
    -DIRECTION INPUT


set_io SDIF0_PERST_N  \
    -pinname P18      \
    -fixed yes        \
    -DIRECTION INPUT


set_io SWITCH         \
    -pinname J18      \
    -fixed yes        \
    -DIRECTION INPUT



# 
# Dedicated Peripheral I/O Settings
# 


# 
# Unlocked I/O settings
# The I/Os in this section are unplaced or placed but are not locked
# the other listed attributes have been applied
# 

